Switch>enable

Switch#config ter

Enter configuration commands, one per line. End with CNTL/Z.

Switch(config)#vlan 50

Switch(config-vlan)#name FC

Switch(config-vlan)#vlan 70

Switch(config-vlan)#name FCL

Switch(config-vlan)#vlan 90

Switch(config-vlan)#name FCIS

Switch(config-vlan)#ECIT

^

% Invalid input detected at '^' marker.

Switch(config-vlan)#EXIT

Switch(config)#int rang fa0/1-4

Switch(config-if-range)#sw mode trunk

Switch(config-if-range)#exit

Switch(config)#exit

Switch#

%SYS-5-CONFIG\_I: Configured from console by console

Switch#vlan brief

^

% Invalid input detected at '^' marker.

Switch#sh vlan brief

VLAN Name Status Ports

---- -------------------------------- --------- -------------------------------

1 default active Fa0/1, Fa0/2, Fa0/3, Fa0/4

Fa0/5, Fa0/6, Fa0/7, Fa0/8

Fa0/9, Fa0/10, Fa0/11, Fa0/12

Fa0/13, Fa0/14, Fa0/15, Fa0/16

Fa0/17, Fa0/18, Fa0/19, Fa0/20

Fa0/21, Fa0/22, Fa0/23, Fa0/24

50 FC active

70 FCL active

90 FCIS active

1002 fddi-default active

1003 token-ring-default active

1004 fddinet-default active

1005 trnet-default active

Switch#copy running-config startup-config

Destination filename [startup-config]?

Building configuration...

[OK]

Switch#enable

Switch#conf ter

Enter configuration commands, one per line. End with CNTL/Z.

Switch(config)#VLAN

% Incomplete command.

Switch(config)#VLAN 50

Switch(config-vlan)#name FC

Switch(config-vlan)#VLAN 70

Switch(config-vlan)#name FCL

Switch(config-vlan)#VLAN 90

Switch(config-vlan)#VALN FCIS

^

% Invalid input detected at '^' marker.

Switch(config-vlan)#NAME FCIS

Switch(config-vlan)#exit

Switch(config)#int ran fa0/1-5

Switch(config-if-range)#sw mode access

Switch(config-if-range)#sw access VLAN 50

Switch(config-if-range)#int rang fa0/6-10

Switch(config-if-range)#sw mode access

Switch(config-if-range)#sw access VLAN 70

Switch(config-if-range)#int rang fa0/11-23

Switch(config-if-range)#sw mode access

Switch(config-if-range)#sw acceess VALN 90

^

% Invalid input detected at '^' marker.

Switch(config-if-range)#sw acceess VLAN 90

^

% Invalid input detected at '^' marker.

Switch(config-if-range)#sw access VLAN 90

Switch(config-if-range)#EXIT

Switch(config)#int fa0/24

Switch(config-if)#sw mode trunk

Switch(config-if)#exit

Switch(config)#exit

Switch#

%SYS-5-CONFIG\_I: Configured from console by console

Switch#sh valn brief

^

% Invalid input detected at '^' marker.

Switch#sh vlan brief

VLAN Name Status Ports

---- -------------------------------- --------- -------------------------------

1 default active Fa0/24

50 FC active Fa0/1, Fa0/2, Fa0/3, Fa0/4

Fa0/5

70 FCL active Fa0/6, Fa0/7, Fa0/8, Fa0/9

Fa0/10

90 FCIS active Fa0/11, Fa0/12, Fa0/13, Fa0/14

Fa0/15, Fa0/16, Fa0/17, Fa0/18

Fa0/19, Fa0/20, Fa0/21, Fa0/22

Fa0/23

1002 fddi-default active

1003 token-ring-default active

1004 fddinet-default active

1005 trnet-default active

Switch#

Switch#copy running-config startup-config

Destination filename [startup-config]?

Building configuration...

[OK]

Switch#